Project Report

1. Clock cycles used 84 for complete execution and each timestamp is evaluated in 6 clock cycle in which (2(1 cc to set the control values and other to reset control values) cycles for multiplexer and input latch while 2 cycles were used for execution of addition/multiplication and 2 cycles were used for demultiplexer and latch)